**To install classic, simply use the following command:**

sudo snap install classic --beta --devmode

**change the permissions of GPIO so that we don’t need sudo (this will be reset upon reboot):**

$ sudo chmod a+rw /dev/gpiomem

**install i2c:**

sudo apt-get install -y python-smbus

sudo apt install i2c-tools

Create an I2C usergroup, apply it to the bus and add your user to this group:

sudo groupadd i2c (group may exist already)

sudo chown :i2c /dev/i2c-1 (or i2c-0)

sudo chmod g+rw /dev/i2c-1

sudo usermod -aG i2c \*INSERT YOUR USERNAME\*

Log out and log in. I was connected via VS code's SSH extension and needed to reboot. Then retry:

i2cdetect -y 1